## Assignment -4

|  |  |
| --- | --- |
| Assignment Date | 29 October 2022 |
| Student Name | BOOMADEVI M |
| Student Roll Number | 95071914019 |
| Maximum Marks | 2 Marks |

**Question-1:**

# Write code and connections in wokwi for the ultrasonic sensor.

Whenever the distance is less than 100 cms send an "alert" to the IBM cloud and display in the device recent events.

# Upload document with wokwi share link and images of IBM cloud

## Solution :

#include <WiFi.h> #include <PubSubClient.h> #include <ArduinoJson.h>

WiFiClient wifiClient;

#define ORG "nhpwjc"

#define DEVICE\_TYPE "raspberypi" #define DEVICE\_ID "12345"

#define TOKEN "123456789"

#define speed 0.034 char server[] = ORG

".messaging.internetofthings.ibmcloud.com"; char

publishTopic[] = "iot-2/evt/Data/fmt/json"; char topic[] = "iot-2/cmd/home/fmt/String"; char authMethod[] = "use-token- auth"; char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, wifiClient); void publishData();

const int trigpin=5; const int echopin=18;

String command; String data="";

long duration; int dist;

void setup()

{

**Serial**.begin(115200); pinMode(trigpin, OUTPUT); pinMode(echopin, INPUT); wifiConnect(); mqttConnect();

}

void loop() { publishData();

delay(500);

if (!client.loop()) { mqttConnect();

}

}

void wifiConnect() {

**Serial**.print("Connecting to "); **Serial**.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6); while (WiFi.status()

!= WL\_CONNECTED) {

delay(500);

**Serial**.print(".");

}

**Serial**.print("WiFi connected, IP address: "); **Serial**.println(WiFi.localIP());

}

void mqttConnect() {

if (!client.connected()) {

**Serial**.print("Reconnecting MQTT client to "); **Serial**.println(server); while (!client.connect(clientId, authMethod, token)) { **Serial**.print("."); delay(1000);

}

initManagedDevice();

**Serial**.println();

}

}

void initManagedDevice() {

if (client.subscribe(topic)) { **Serial**.println(client.subscribe(topic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

} } void publishData()

{ digitalWrite(trigpin,LOW); digitalWrite(trigpin,HIGH); delayMicroseconds(10); digitalWrite(trigpin,LOW); duration=pulseIn(echopin,HIGH); dist=duration\*speed/2;

if(dist<100){

DynamicJsonDocument doc(1024); String payload;

doc["AlertDistance:"]=dist; serializeJson(doc, payload); delay(3000); **Serial**.print("\n");

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");


} else {


**Serial**.println("Publish FAILED");

}

}

}





# 